**Wetland Setback Regulation**

The minimum setback to wetlands, bordering vegetative wetlands, and Waterways shall be 50 feet from the soil absorption system. Any distance measuring 50 to 100 feet from a wetland, watercourse, or bordering vegetative wetland requires a variance from the Board of Health. That Septic System design shall have an alternative system design able to treat water for Nitrates. Filling or replicating wetlands in order to attain minimal required setback is prohibited.

***Amended March 19, 1997 Published February 27 and March 6, 1997***

***Amended January 12, 2022 Published January 20, 2022***

***Amended 03/02/2022 Published 03/10/2022 –*** ***The Wanderer***